SIMULATION FUNCTION [SJ6A-EL]

id050208100800

• By using the Mazda Modular Diagnostic System (M-MDS), simulation items for input/output parts preset in the TCM can be optionally selected and operated regardless of TCM control conditions.

Simulation Item Table

X: Available

Simulation item | Applicable component | Unit/Condition | Operation | TCM terminal
--- | --- | --- | --- | ---
IG ON | Idle
LPS | Line pressure control solenoid | A | N/A | X | 1E, 1R
SSA | Shift solenoid A | On/Off | N/A | X | 1AF
SSB | Shift solenoid B | On/Off | N/A | X | 1AB
SSC | Shift solenoid C | On/Off | N/A | X | 1AA
SSD | Shift solenoid D | On/Off | N/A | X | 1S
SSE | Shift solenoid E | On/Off | N/A | X | 1V
SSF | Shift solenoid F | A | N/A | X | 1O, 1Z
SSG | Shift solenoid G | A | N/A | X | 1L, 1Y
TCCC | TCC control solenoid | A | N/A | X | 1D, 1Q