DISCHARGE HEADLIGHT CONTROL MODULE CONSTRUCTION/OPERATION

id091800103300

  Warning
  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the discharge headlight service warnings. (See MX-5 Workshop Manual.)

• Built into the front combination light and installed on the front combination light lower side.

amxzzn00000541

• Switches the direct current from the battery to alternating current (25,000 V) and optimally controls the current supply output to the discharge headlight.