FRONT UPPER ARM CONSTRUCTION

id021300629800

• The front upper arm is made of aluminum for improved rigidity and weight reduction.
• The zero-stopper-clearance rubber bushings have been adopted for where the upper arm attaches to the front crossmember.

  ― The stopper sleeve, integrated with the inner pipe, protrudes slightly.
  ― This structure suppresses forward-backward movement caused by external forces acting on the arm.
  ― It also enables linear spring characteristics of the bushings from an early stage, thereby optimizing control over changes in vehicle behavior.

amxzzn00000297