DSC OFF SWITCH, DSC OFF LIGHT OPERATION

id041500102700

• When the DSC system and CAN lines are functionally normally, the DSC OFF light illuminates for approx. 3 s when the ignition switch is turned to the ON position to check the light function.
• When the DSC OFF switch is pressed to disable DSC control, the DSC OFF light illuminates.

  Note
  • When releasing the DSC, continue to press the DSC OFF switch until the DSC OFF light illuminates.

amxzzn00000714