CYLINDER HEAD COVER CONSTRUCTION [L8, LF]

id0110a9100200

• The cylinder head cover is made of integrated plastic, which is lightweight and sound absorbent.
• The oil filler cap is a bayonet type.
• The boss for installing the camshaft position (CMP) sensor is provided at the rear of the cylinder head cover.
• LF engine models has a hole for installing the oil control valve (OCV).
• A dipstick insertion hole has been equipped to the cylinder head cover.

amxzzn00000444