REAR ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION

id041300800500

1. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

2. Remove the partition board. (See PARTITION BOARD REMOVAL/INSTALLATION.)

3. Remove the trunk side trim. (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove the fuel-filler pipe protector. (See FUEL TANK REMOVAL/INSTALLATION [L8, LF].)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

amxzzw00000255

1 | Connector
2 | Bolt
3 | Rear ABS wheel-speed sensor