FRONT BODY STRAIGHT-LINE DIMENSIONS (2) [DIMENSIONS]

id098010740700

amxzzb00000017

amxzzb00000018

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
A | Bonnet hinge installation hole | ø12 {0.47}
B | Front fender installation hole | ø7 {0.28}
C | Suspension housing upper datum hole | ø13 {0.51}
D | Front fender installation hole | ø10 {0.39}
E | Front bumper installation hole | ø7 {0.28}