HANDS-FREE TELEPHONE (HF/TEL) SYSTEM OPERATION

id092000834600

• Calls and mobile phone operation can be made without operating the Bluetooth-enabled mobile phone directly. The functions vary depending on the corresponding profile.

Hands-free Telephone (HF/TEL) System Operation

• The HF/TEL unit sends the information from the Bluetooth-enabled mobile phone to the center panel unit. Then, the center panel unit outputs the audio data to the speakers and the display shows the information.
• The operation for answering an incoming call/making an outgoing call can be performed using the audio control switches. When an audio control switch is operated, its operation information is sent to the HF/TEL unit via the center panel unit, then to the Bluetooth-enabled mobile phone.
• Voice from a phone receiver is output from the door speaker. Voice spoken into the vehicle’s microphone is sent to the Bluetooth-enabled device by the HF/TEL unit.

amxzzn00000276