INSTRUMENTATION/DRIVER INFO. PERSONALIZATION FEATURES SETTING PROCEDURE

id092200889900

  Note
  • Use the IDS (laptop PC) because the PDS (Pocket PC) does not support the INSTRUMENT CLUSTER CUSTOMIZED FUNCTION SETTING PROCEDURE.

1. Connect the M-MDS to the DLC‐2.

amxzzw00001703

2. After the vehicle is identified, select the following items from the initial screen of the M-MDS.

  1. Select the “Module Programming”.

3. Then, select items from the screen menu in the following order.

  1. Select “Programmable Parameters”.
  2. Select “Warning Lamps / Chimes”.

4. Select an item name, and then select option.

  Items

  • Fuel logic (Disabled / Enabled)
  • DIS Correction (-15%, -10%, -5%, 0%, 5%, 10%, 15%)