NO.3 THERE IS A MALFUNCTION IN THE SYSTEM EVEN THOUGH ABS WARNING LIGHT, BRAKE SYSTEM WARNING LIGHT, DSC INDICATOR LIGHT AND DSC OFF LIGHT DO NOT ILLUMINATE [DYNAMIC STABILITY CONTROL (DSC)]

id0403b2805500

3 | There is a malfunction in the system even though ABS warning light, brake system warning light, DSC indicator light and DSC OFF light do not illuminate
--- | ---
POSSIBLE CAUSE | • There is a mechanical malfunction in system ― DSC HU/CM DTC is stored ― DSC system malfunction ― Conventional brake system malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | CONFIRM DSC HU/CM DTC • Perform the Reading DTCs Procedure. (See ON-BOARD DIAGNOSIS [DYNAMIC STABILITY CONTROL (DSC)].) • Are any DTC present? | Yes | Go the applicable DTC inspection. (See ON-BOARD DIAGNOSIS [DYNAMIC STABILITY CONTROL (DSC)].)
No | Go to the next step.
2 | INSPECT DSC SYSTEM • Perform “DSC SYSTEM INSPECTION”. (See DSC SYSTEM INSPECTION.) • Is there any malfunction? | Yes | Repair or replace the malfunctioning part according to the inspection results.
No | Inspect the conventional brake system. Repair or replace the malfunctioning part according to the inspection results, if necessary.