FRONT BODY STRAIGHT-LINE DIMENSIONS (1) [DIMENSIONS]

id098010740600

amxzzb00000015

amxzzb00000016

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
A | Front header notch | -
B | Front header projection location | -
C | Front fender installation slot | ø10 x 12
{0.39 x 0.47}
D | Front combination light installation hole | ø7 {0.28}
E | Front combination light installation hole | ø7 {0.28}
F | Front bumper reinforcement installation hole | ø14 {0.55}
G | Bonnet bracket datum hole | ø10 {0.39}
G’ | Bonnet bracket datum slot | ø10 x 14
{0.39 x 0.55}