CLIMATE CONTROL UNIT REMOVAL/INSTALLATION [MANUAL AIR CONDITIONER]

id0740a2807400

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the side wall. (See SIDE WALL REMOVAL/INSTALLATION.)

4. Remove the center panel unit. (See CENTER PANEL UNIT REMOVAL/INSTALLATION.)

5. Remove the climate control unit from the center panel unit.

e5u740zw5105

6. Install in the reverse order of removal.