DRIVE BELT CONSTRUCTION [L8, LF]

id0110a9102500

• The single, serpentine type drive belt drives auxiliary parts, resulting in a shortened overall engine length and improved serviceability.
• A drive belt auto tensioner with an embedded coil spring has been adopted to automatically maintain the optimal drive belt tension.

Drive Belt Specification.

item | Specification
--- | ---
L8, LF
Belt length | mm {in} | About 2,243 {88.31} (About 2,163 {85.16})*
Belt width | mm {in} | About 20.5 {0.81}

* : A/C non-equipping vehicle specification.

amxzzn00000473