SIDE STEP MOLDING REMOVAL

id091600804400

1. Remove the fasteners.

e5u916zw5003

2. Pull the side step molding and remove clips A from the body.

3. Slide the side step molding to the vehicle rear and remove clips B and C from the side step molding.

4. Remove the side step molding.

5. Remove clips B and C from the body, then install it to the side step molding.

6. Install in the reverse order of removal.