CLIMATE CONTROL UNIT CONSTRUCTION [MANUAL AIR CONDITIONER]

id0740a2100900

• Composed of the following parts:

  ― Fan switch
  ― Airflow mode control dial
  ― REC switch
  ― A/C switch
  ― Temperature control dial
  ― Rear window defroster switch

amxzzn00000412

• Hot or cold air is blown from the waist louver beside the audio when any mode position (OPEN-VENT, OPEN-BI-LEVEL, OPEN-HEAT) is selected.

amxzzn00000413