ELECTRICAL SYSTEM

id000000157000

Connectors

Disconnecting connectors

  • When disconnecting connector, grasp the connectors, not the wires.

  belbze00000024

  • Connectors can be disconnected by pressing or pulling the lock lever as shown.

  belbze00000025

Locking connector

  • When locking connectors, listen for a click indicating they are securely locked.

  belbze00000026

Inspection

  • When a tester is used to inspect for continuity or measuring voltage, insert the tester probe from the wiring harness side.

  belbze00000027

  • Inspect the terminals of waterproof connectors from the connector side since they cannot be accessed from the wiring harness side.
    Caution
    • To prevent damage to the terminal, wrap a thin wire around the tester probe before inserting into terminal.

  belbze00000028