OIL PUMP DISASSEMBLY

id051300260300

Components

bsj6za00000537

1 | Pump housing
2 | O-ring
3 | Outer oil pump gear
4 | Inner oil pump gear
5 | Oil pump shaft
6 | O-ring
7 | Seal ring
8 | Bearing race
9 | Thrust needle bearing
10 | Oil seal

Disassembly

1. Remove the O-ring from the oil pump component.

bsj6za00000602

2. Remove the seal ring from the oil pump shaft.

bsj6za00000603

3. Put an installation mark on the pump housing and oil pump shaft.

bsj6za00000778

4. Remove the screw from the oil pump.

bsj6za00000604

5. Remove the oil pump shaft from the pump housing.

bsj6za00000605

6. Remove the O-ring from the pump housing.

bsj6za00000577

7. Remove the inner oil pump gear and outer oil pump gear from the pump housing.

bsj6za00000606

8. Using a flathead screwdriver, remove the oil seal from the pump housing.

bsj6za00000122

  Caution
  • Do not damage the bushing on the pump housing.