FRONT BODY STRAIGHT-LINE DIMENSIONS (3) [DIMENSIONS]

id098010740800

amxzzb00000019

amxzzb00000020

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
A | Front header notch | -
B | Wiper installation hole | ø7 {0.28}
C | Bonnet hinge installation hole | ø12 {0.47}
D | Front fender installation hole | ø7 {0.28}
E | Suspension mounting reinforcement datum hole | ø8.2 {0.32}
F | Front fender installation hole | ø10 {0.39}
G | Front side frame outer datum slot | ø10 x 14
{0.39 x 0.55}