DIRECT MODE CONTROL OUTLINE [SJ6A-EL]

id051311638000

Features

• Direct mode control enables temporary use of manual shifting using the steering shift switch even when the selector lever is in the D range.
• The transmission can be controlled at the driver's discretion by operating the steering shift switch, which enables effective downshift during deceleration using engine brake force, cornering after deceleration, and acceleration when passing.
• After switching to direct mode, the system returns to automatic shift mode automatically in accordance with driving conditions.

Block Diagram

amxzzn00000708

System Flow

ar8wzn00000504