BRAKE SWITCH INSPECTION

id041100801900

  Caution
  • If the brake switch is removed from the brake pedal (MT) or the interlock unit (AT), its proper functioning cannot be guaranteed when reinstalled. Therefore, inspect the brake switch with it still installed, or replace the brake switch if it is removed.

1. Verify continuity as indicated in the table.

  • If not as indicated in the table, replace the brake switch.

amxzzw00002540

amxzzw00002541