SUPER-LSD CONSTRUCTION

id031400100400

• Inside the super-LSD, taper rings that are fixed to the differential gear case have been placed between the differential gear case and the side gears. Additionally, a cone is provided around the outer surface of the side gear.
• Springs and retainers are positioned between the right and left side gears to provide initial torque to the taper rings.

amxzzn00000436