SIMULATION TEST [L8, LF]

id0102b1100600

• The simulation items are shown below.

Simulation item table

×: Applicable
—: Not applicable

Item | Applicable component | Unit/condition | Test condition | PCM terminal
--- | --- | --- | --- | ---
KOEO | KOER
ACCS | A/C relay | Off/On | × | × | 1I
ALTF | Generator (field coil) | OFF/ON | — | × | 2AI
ARPMDES | Target engine speed | RPM | × | × | —
EVAPCP | Purge solenoid valve | % | × | × | 2C
FAN1 | Cooling fan relay No.1 | Off/On | × | × | 1M
FAN2 | Cooling fan relay No.2 | Off/On | × | × | 1N
FAN3 | Cooling fan relay No.3 | Off/On | × | × | 1R
FP | Fuel pump relay | Off/On | × | × | 1H
FUELPW1 | Fuel injector | % | × | × | 2BB, 2BC, 2BD, 2AZ
GENVDSD | Target generator voltage | V | — | × | —
HTR11 | A/F sensor heater | Off/On | × | × | 2BG
HTR12 | HO2S heater | Off/On | × | × | 2BE
IMRC | Variable tumble solenoid valve | Off/On | × | × | 2I
IMTV | Variable intake air solenoid valve | Off/On | × | × | 2J
INJ_1 | Fuel injector No.1 | OFF | — | × | 2BB
INJ_2 | Fuel injector No.2 | OFF | — | × | 2BC
INJ_3 | Fuel injector No.3 | OFF | — | × | 2BD
INJ_4 | Fuel injector No.4 | OFF | — | × | 2AZ
SEGRP | EGR valve stepping motor position | — | × | × | 2K, 2G, 2L, 2H
test | Test mode | Off/On | × | × | —
VT DUTY1 Wt*1 | CMP sensor | % | × | × | 2E

*1 :With variable valve timing mechanism