UNDERBODY FLAT-PLANE DIMENSIONS [DIMENSIONS]

id098010740400

• The following figures are bottom and side views.

d5u0980b001

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
A | Front side frame datum hole | ø7 {0.28}
B | Crossmember No.1 datum hole | ø7 {0.28}
C | Engine mounting bolt | M14 {0.55}
D | Front suspension mounting block | ø64 {2.52}
E | Engine mounting bolt | M14 {0.55}
F | Front frame rear datum hole | ø16 {0.63}
G | Front frame rear datum slot | ø16 x 20
{0.63 x 0.79}
H | Front B frame datum hole | ø12 {0.47}
I | Front B frame datum slot | ø12 x 18
{0.47 x 0.71}
J | Rear side frame datum hole | ø16 {0.63}
K | Rear crossmember mounting bolt | M14 {0.55}
L | Rear crossmember mounting bolt | M14 {0.55}
M | Rear suspension mounting block | ø97 {3.82}
N | Rear crossmember mounting bolt | M14 {0.55}
O | Rear side frame datum slot | ø16 x 20
{0.63 x 0.79}