NO.6 DISC CHANGE IS INOPERATIVE [CD PLAYER/CHANGER]

id0903e5806400

6 | Disc change is inoperative
--- | ---
Possible DTC | 22:Er01
POSSIBLE CAUSE | • Improper center panel installation • Audio unit malfunctioning • Center panel malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Inspect the CD changer operation. • Does the CD changer operate properly? | Yes | Go to the next step.
No | Go to the symptom troubleshooting “No.3 CD player/changer does not play the CD/No sound”.
2 | • Inspect the followings: ― Is the display shown properly when operating the disc change button? ― Does the radio band selection operate properly? | Yes | Replace the audio unit. (See CENTER PANEL UNIT REMOVAL/INSTALLATION). (See CENTER PANEL UNIT DISASSEMBLY/ASSEMBLY).
No | Go to the next step.
3 | • Inspect the center panel installation. • Does the CD changer change the disc properly after re-installing the center panel? | Yes | Install the center panel securely and properly.
No | Go to the “No.1 center panel switch inspection” in this section. Replace the center panel as necessary.