RESTRAINTS FEATURES

id080000100200

Improved safety | • A driver-side air bag module has been adopted. • A passenger-side air bag module has been adopted. • A side air bag module has been adopted. • Three-point seat belt with the following functions for seat passengers adopted ― ELR (Emergency Locking Retractor: emergency locking mechanism) ― Pre-tensioner seat belt (See PRE-TENSIONER SEAT BELT CONSTRUCTION/OPERATION.) ― Load limiter, which adjusts restraint force of the seat belt to reduce the possibility of injury to passengers caused by excess seat belt pressure after pre-tensioner operation • The active bonnet has been adopted. (European (L.H.D. U.K.) specs.)