DTC B1342 [POWER RETRACTABLE HARDTOP]

id0902j2920500

DTC B1342 | Power retractable hardtop control module internal malfunction
--- | ---
POSSIBLE CAUSE | • Malfunction in the power retractable hardtop control module internal circuit

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT THE POWER RETRACTABLE HARDTOP CONTROL MODULE • Clear the DTC from the power retractable hardtop control module memory using the M-MDS. • Turn the ignition switch to the ON position. • Is the DTC displayed? ― B1342 | Yes | Replace the power retractable hardtop control module. (See POWER RETRACTABLE HARDTOP CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.