OIL PRESSURE GAUGE CONTROL CONSTRUCTION/OPERATION

id092200111800

System Wiring Diagram

amxzzn00000503

Operation

• The engine coolant temperature signal and engine speed signal sent from the PCM via the CAN system is input to the microcomputer in the instrument cluster. The microcomputer calculates the oil pressure based on the engine coolant temperature signal and engine speed signal, and sends the output signal to the oil pressure gauge according to the calculated value.