HVAC FEATURES

id070000100200

Reduced weight | • Integrated A/C unit adopted
Improved air conditioning performance | • Sub-cooling system to multi-flow condenser adopted
Improved comfort | • Open mode has been added to the air flow mode
Reduced fuel consumption when the A/C is operating (Reduced idling increase amount when A/C compressor is operating) | • Refrigerant pressure switch with medium-pressure switch adopted
Improved operability | • Climate control unit with enlarged operation dial and switch adopted