#
INPUT/OUTPUT CHECK MODE OPERATION

id092200100900

## Input Circuit Check

• When the parts listed in the chart are operated and signal is output to the instrument cluster, the built-in microcomputer determines the operability of the input circuit based on that signal.

No. | Parts sending input signal
--- | ---
04 | Door switch
08 | TNS relay
22 | Fuel gauge sender unit
31 | Key reminder switch

## Individual Circuit Check

• By operating the parts listed in the chart, the built-in microcomputer determines the operability of the individual parts.

No. | Parts sending input signal
--- | ---
12 | Speedometer
13 | Tachometer
14 | Buzzer
16 | Fuel-level warning light
23 | Fuel gauge
25 | Water temperature gauge
26 | LCD