#
PRIMARY GEAR DISASSEMBLY/ASSEMBLY

id051700116600

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Bearing (See Bearing Disassembly Note.) (See Bearing Assembly Note.)
2 | Primary gear

## Bearing Disassembly Note

• Remove the bearing from the primary gear using the SSTs and suitable plate.

## Bearing Assembly Note

• Install the bearing to the primary gear using the SSTs.