#
DRIVELINE/AXLE SPECIFICATIONS

id030000100200

Item | Specification
--- | ---
Engine type | ZJ | ZY
Front axle | Bearing type | Angular ball bearing
Rear axle | Bearing type | Taper roller bearing (unit-type)
Drive shaft | Joint type | Wheel side | Bell joint
Differential side | Tripod joint
Shaft diameter | (mm {in}) | 21.8 {0.86} | 21.8 {0.86} (MTX) 22.8 {0.90} (ATX)
Joint shaft | Shaft diameter | (mm {in}) | 26.0 {1.02}