#
COWL GRILLE REMOVAL/INSTALLATION

id091600444000

1. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

1 | Weatherstrip
2 | Cowl grille (LH)
3 | Cowl grille (RH) (See Cowl Grille (RH) Removal Note)

3. Install in the reverse order of removal.

## Cowl Grille (RH) Removal Note

1. Pull the cowl grille toward vehicle front, and remove the clip from the pin (cowl panel).

2. Remove the cowl grille.