CYLINDER HEAD ASSEMBLY (I)

id011000504300

1. Assemble in the order indicated in the table.

bezeze00000054

1 | Valve seal (See Valve Seal Assembly Note.)
2 | Valve
3 | Valve spring
4 | Upper valve spring seat
5 | Valve keeper (See Valve Keeper Assembly Note.)

Valve Seal Assembly Note

1. Press in the valve seal to the valve guide by hand.

2. Install the valve seal using the SST.

bezeze00000055

Valve Keeper Assembly Note

1. Install the valve keeper using the SST.

bezeze00000056