#
STEERING SPECIFICATIONS

id060000100300

Item | Specification
--- | ---
Steering wheel | Outer diameter | mm {in} | 372 {14.6}
Lock-to-lock | (turns) | 2.7
Steering gear and linkage | Type | Rack-and-pinion
Rack stroke | mm {in} | 147.4 {5.8}
Steering column and shaft | Shaft type | Collapsible
Joint type | 2-cross joint
Amount of tilt | mm {in} | 46 {1.8}
Power steering system | Power assist type | Engine speed sensing
Power steering fluid | Type | M-III or equivalent (e.g. Dexron®II)
Fluid capacity* (approximate quantity) (L {US qt, Imp qt}) | 1.05 {1.11, 0.92}

  * :
When fluid reservoir tank is at maximum volume.