#
DTC B2477

id0802a0810500

DTC B2477 | Configuration error
--- | ---
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection with only detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • SAS control module configuration has not been performed correctly
POSSIBLE CAUSE | • SAS control module configuration error • SAS control module malfunction

Diagnostic procedure

Inspection | Action
--- | ---
CONFIGRATION • Using the WDS or equivalent, perform SAS control module configuration. (SeeSAS CONTROL MODULE CONFIGURATION.) • Is DTC B2477 indicated? | Yes | [Present malfunction diagnosis] Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.) [Past malfunction diagnosis] Troubleshooting completed.
No | Troubleshooting completed.