#
CENTER PANEL MODULE REMOVAL/INSTALLATION

id092000804600

1. Disconnect the negative battery cable.

2. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Knob
2 | Screw
3 | Bolt
4 | Center panel module (See Center Panel Module Removal Note)
5 | Connector
6 | Antenna feeder

4. Install in the reverse order of removal.

  Caution

  • When installing the center panel module, make sure that the wiring harness and antenna feeder are not caught between the unit and dashboard. If the harness or the antenna feeder is caught between the unit and dashboard, it may cause malfunctions.

## Center Panel Module Removal Note

1. Remove the ashtray.

2. Pull the center panel module outward from the underside.

3. Disengage clips A from the dashboard and remove the center panel module.