#
ENTERTAINMENT OUTLINE

id092000100100
• A center panel module composed of the installed audio unit with the audio switch, A/C switch, hazard warning switch and rear window defroster switch built into the center panel has been adopted.
• The audio unit consists of the following parts:

  - Base unit, which has AM/FM tuner and control function for each module
  - Upper module (CD player or CD changer)
  - Lower module (cassette deck or MD player)
  - Cover

• An upper module (CD player or CD changer) and lower module (cassette deck or MD player) are options.
• Module availability depends on vehicle grade.
• The audio control switch is equipped on the steering wheel for audio operation.
• A center roof antenna has been adopted.
• Four speakers installed as standard, one each to the front and rear doors, have been adopted.
• All information related to the audio system appears on the center panel LCD.