#
NO.25 ENGINE STALLS WHEN DRIVING AT SLOW SPEEDS OR STOPPING [FN4A-EL]

id0503a1805800

25 | Engine stalls when driving at slow speeds or stopping
DESCRIPTION | • Engine stalls when brake pedal is depressed while driving at low speed or stopping.
POSSIBLE CAUSE | • The malfunction on engine control side (e.g. Fuel injection control, IAC system) Otherwise, the malfunction is in the control valve body, shift solenoid E or TCC.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Go to symptom troubleshooting No.10 "LOW IDLE/STALLS DURING DECELERATION". (See NO.10 LOW IDLE/STALLS DURING DECELERATION [WITHOUT WU-TWC].) (See NO.10 LOW IDLE/STALLS DURING DECELERATION [WITH WU-TWC].) • Does engine control system normal? | Yes | Go to next step.
No | Repair or replace any defective parts according to inspection results.
2 | • Go to symptom troubleshooting No.5 "ENGINE STALLS-AFTER START/AT IDLE." (See NO.5 ENGINE STALLS-AFTER START/AT IDLE [WITHOUT WU-TWC].) (See NO.5 ENGINE STALLS-AFTER START/AT IDLE [WITH WU-TWC].) • Is engine control system normal? | Yes | Repeat basic inspection and repair or replace any defective parts according to inspection result. (See BASIC INSPECTION [FN4A-EL].)
No | Repair or replace any defective parts according to inspection results.
3 | • Verify test results. - If normal, return to diagnostic index to service any additional symptoms. - If malfunction remains, inspect related Service Information and perform repair or diagnosis. • If vehicle repaired, troubleshooting completed. • If vehicle not repaired or additional diagnostic information not available, replace PCM.