#
EMISSION SYSTEM OUTLINE [WITHOUT WU-TWC]

id0116001001d0
• The construction and operation of the emission system is essentially carried over from that of the previous Mazda 121 121DEMIO (DW) models.
×: Applicable
-: Not applicable

Item | Mazda2 (DY) | Previous Mazda 121 121DEMIO (DW) | Remark for new model
--- | --- | --- | ---
ZJ | ZY
PCV valve | × | Same function as previous Mazda 121 121DEMIO (DW) models
Purge solenoid valve | × | Same function as previous Mazda 121 121DEMIO (DW) models
Charcoal canister | × | Same function as previous Mazda 121 121DEMIO (DW) models
Rollover valve | × | Same function as previous Mazda 121 121DEMIO (DW) models
Evaporative gas check valve (One-way) | × | Same function as previous Mazda 121 121DEMIO (DW) models
TWC | × | Same function as previous Mazda 121 121DEMIO (DW) models