#
CONTROL SYSTEM

id074000803600

1 | Blower motor (See BLOWER MOTOR REMOVAL/INSTALLATION) (See BLOWER MOTOR INSPECTION)
2 | Resistor (See RESISTOR REMOVAL/INSTALLATION) (See RESISTOR INSPECTION)
3 | Magnetic clutch (See MAGNETIC CLUTCH DISASSEMBLY/ASSEMBLY) (See MAGNETIC CLUTCH ADJUSTMENT) (See MAGNETIC CLUTCH INSPECTION)
4 | Evaporator temperature sensor (See EVAPORATOR TEMPERATURE SENSOR REMOVAL/INSTALLATION) (See EVAPORATOR TEMPERATURE SENSOR INSPECTION)
5 | Refrigerant pressure switch (See REFRIGERANT PRESSURE SWITCH REMOVAL/INSTALLATION) (See REFRIGERANT PRESSURE SWITCH INSPECTION)
6 | Climate control unit (See CLIMATE CONTROL UNIT REMOVAL) (See CLIMATE CONTROL UNIT INSTALLATION) (See CLIMATE CONTROL UNIT DISASSEMBLY/ASSEMBLY) (See CLIMATE CONTROL UNIT WIRE ADJUSTMENT)
7 | A/C relay (See RELAY INSPECTION)
8 | Blower relay (See RELAY INSPECTION)
9 | PCM (See PCM INSPECTION [WITHOUT WU-TWC]) (See PCM INSPECTION [WITH WU-TWC])
10 | Rear window defroster relay (See RELAY INSPECTION)