#
AUDIO SYSTEM SPECIFICATIONS

id092000100400

## Audio Unit

Item | Specification
--- | ---
Australian specs. | General (R.H.D.) specs.
Rated voltage | (V) | 12
Frequency band | AM | (kHz) | 522-1629 530-1620 | 522-1629
FM | (MHz) | 87.5-108.0
Audio amplifier maximum output power | (W) | 25×4
Output impedance | (ohm) | 4

## Speaker

Item | Specification
--- | ---
Door speaker
Maximum input | (W) | 25
Impedance | (ohm) | 4
Lowest resonance level | (Hz) | 85
Sound pressure level | (dB) | 85
Size | (cm) | 16