#
QUICK RELEASE CONNECTOR

id011400102600

## Outline

• The function of the quick release connector is essentially carried over from that of the current Mazda6 (GG, GY) L3 engine models, except for the following:

  - A lock clip has been adopted on the engine compartment side.
  - A shortened-type quick release connector has been adopted for the fuel pump.

## Structure

### Engine compartment side

  • The quick release connector on the engine compartment side has a lock clip to prevent disconnection. After the quick release connector is connected, the quick release connector is protected from unexpected disconnection by the locking of the lock clip inner guide.

### Fuel tank side (fuel pump part)

  • The fuel pump quick release connector has adopted a shortened-type quick release connector allowing connection of a short fuel pipe. Connection of a short fuel pipe is possible by the shortening of length (A) from the quick release connector end to the lock point. Because the length (A) to the lock point is shortened, the checker tab is located on the fuel hose side. The disconnect/connect procedure is the same as that of the quick release connector on the fuel tank side except for the fuel pump.