#
HIGH-MOUNT BRAKE LIGHT REMOVAL/INSTALLATION

id091800802000

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Cover
2 | Connector
3 | Socket
4 | High-mount brake light bulb
5 | Fastener
6 | High-mount brake light (See High-mount Brake Light Installation Note)

3. Install in the reverse order of removal.

## High-mount Brake Light Installation Note

1. Pass the wiring harness through the high-mount brake light hole, then install the light to the liftgate.