#
FOREWORD

id010200800300
• When the customer reports a vehicle malfunction, check the malfunction indicator lamp (MIL) indication and diagnostic trouble code (DTC), then diagnose the malfunction according to the following flowchart.

  - If a DTC exists, diagnose the applicable DTC inspection. (See DTC TABLE.)
  - If no DTC exists and the MIL does not illuminate or flash, diagnose the applicable symptom troubleshooting. (See ENGINE SYMPTOM TROUBLESHOOTING.)

  * :
Malfunction Indicator Lamp (MIL), Generator Warning Light, Security Light