#
HEADLIGHT BULB REMOVAL/INSTALLATION

id091800464100

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Connector
2 | Cover
3 | Headlight bulb

  Caution

  • A halogen bulb generates extremely high heat when it is used. If the surface of the bulb is soiled, excessive heat will build up and the life of the bulb will be shortened. When replacing the bulb, hold the metal flange, not the glass.

3. Install in the reverse order of removal.