#
SECURITY LIGHT: DTC 13 (WDS: DTC B2431)

id0902e4632400

DTC 13 (B2431) | ID number programing failure.
--- | ---
POSSIBLE CAUSE | • The procedure fails to program the transponder into PCM

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | VERIFY DTC USING SST • Does WDS indicate DTC B2431? | Yes | Go to Step 3.
No | Go to the next step.
2 | VERIFY DTC USING SST • Does WDS indicate DTC B1600? | Yes | Go to SECURITY LIGHT: DTC 13 (WDS: B1600).
No | Go to the next step.
3 | INSPECT PCM • Erase key ID number using WDS and register key ID number. (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING.) • Using registered key, turn the ignition switch to the ON position. • Does WDS indicate DTC B2431 again? | Yes | Replace PCM and reprogram immobilizer system. (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING.)
No | Troubleshooting is completed.