#
CAN SIGNAL-CHART

id094000000400
OUT: Output (sends signal)
IN: Input (receives signal)

Signal | Multiplex module
--- | ---
PCM | ABS HU/CM | Instrument cluster
Engine speed | OUT | - | IN
Wheel speed (front left/front right/rear left/rear right) | IN | OUT | -
Vehicle speed | OUT | - | IN
ECT | OUT | - | IN
Travelled distance | OUT | - | IN
MIL condition | OUT | - | IN
Generator warning light conditions | OUT | - | IN
Transmission/axle type | OUT | IN | IN
Tire circumference (front/rear) | OUT | IN | -
Desired gear/Change lever position | OUT | - | IN
HOLD switch conditions | OUT | - | IN
Brake system configuration (EBD/ABS) | IN | OUT | IN
Brake system status | ABS | IN | OUT | -
EBD/ABS | - | OUT | IN