#
DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM]

id0902e6837000

DTC | Malfunction location | DTC output module | Page
--- | --- | --- | ---
U0073 | CAN system communication error | PCM | (See DTC U0073, U1900, U2516.)
U0121 | Communication error between the ABS HU/CM and DTC output unit | (See PROCEDURES FOR DETERMINING THE LOCATION OF A MALFUNCTION.)
U0155 | Communication error between the instrument cluster and DTC output unit
U1900 | CAN system communication error | Instrument cluster | (See DTC U0073, U1900, U2516.)
U2516 | CAN system wiring harness open or short circuit
U2523 | Communication error between the PCM and DTC output unit (Engine related signal) | ABS HU/CM (Vehicles with the ABS) | (See PROCEDURES FOR DETERMINING THE LOCATION OF A MALFUNCTION.)