#
SELECTOR LEVER DISASSEMBLY/ASSEMBLY

id051800800900

1. Disassemble in the order shown in the figure.

2. Assemble in the reverse order of disassembly.

1 | Connector (See Connector Disassembly Note.)
2 | Selector lever knob component
3 | Cover
4 | Indicator panel
5 | Selector lever

## Connector Disassembly Note

1. Insert a thin piece of metal from the terminal side of the connector, and press down the terminal locking tab.

2. Pull the terminal out of the connector.