#
INSTRUMENT CLUSTER CONFIGURATION

id092200800300

1. Connect the WDS or equivalent to the DLC-2.

2. Input vehicle information following the directions on the screen.

3. Select "Module Programming".

4. Select "Programmable Module Installation".

5. Select the following items and perform procedures according to directions on the screen.

Items

  • "IC"

6. Retrieve DTCs using the WDS or equivalent, then verify that there is no DTC present.

  • If DTC is present, perform applicable DTC inspection.